|  |
| --- |
| Formsteel |
| Structural Report |
| PS1 – Structural calculation and design report |

|  |
| --- |
| Formsteel  4-25-2019 |



[TOC]

# Geometry

## Basic geometry

Width B = [GableWidth] m

Length L = [Length] m

Height H1 = [WallHeight] m

~~Height H~~~~2~~ ~~= 4.48 m~~~~2~~

Roof Pitch α = [RoofPitch\_deg]deg

Girt spacing Bg = [GirtDistance] m

Purlin spacing Bp = [PurlinDistance] m

Wind post spacing Bwp = [ColumnDistance] m

Rafter length 9.423 m

Toto by somasidal do tabulky, aby to bolo peknenaformatovane

Pismenkazakladnehofontu by malibyt co najmensie a citatelne “10”???

Pointa je vsetkonahustittak aby smemali co najmenejstran a co najhutnejsie data.

## Structural model in 3D environment

Orezatbieleokrajeobrazka aby bol co najvacsi. Este samusimetroskupohrat s farbami aby to nabielompozadivyzeralolepsie. Asibudemepotrebovat 2 sadyfarieb pre 3D grafikuaine pre export.

[3DModelImage]

# Material properties

[MaterialProperties]

# Cross-sections

[CrossSections]

# Member types

[MemberTypes]

# Load

## Basic Parameters

[BasicLoadParameters]

Location: [Location]

Design life: [DesignLife\_Value]

Importance level: [ImportanceClass]

Annual probability of exceedance SLS: [AnnualProbabilitySLS]

Return period SLS: RSLS = [R\_SLS] years

Site elevation E = [SiteElevation] m

## Dead Load

[DeadLoad]

Wall cladding load g c.w = [CCalcul\_1170\_1.DeadLoad\_Wall] kN/m2

Roof cladding load g c.r = [CCalcul\_1170\_1.DeadLoad\_Roof] kN/m2

Additional wall load g a.w = [AdditionalDeadActionWall] kN/m2

Additional roof load g a.r = [AdditionalDeadActionRoof] kN/m2

Total wall load g t.w = [CCalcul\_1170\_1.DeadLoadTotal\_Wall] kN/m2

Total roof load g t.r = [CCalcul\_1170\_1.DeadLoadTotal\_Roof] kN/m2

## Service load

Todo – if necessary

## Live / Imposed Load

Roof live load q l.r = [ImposedActionRoof] kN/m2

[ImposedLoad]

## Snow Load

[SnowLoad]

Annual probability of exceedance ULS: [AnnualProbabilityULS\_Snow]

Return period RULS.S = [R\_ULS\_Snow] years

Snow elevation region: [CCalcul\_1170\_3.eSnowElevationRegion]

Ground snow load sg.ULS= [CCalcul\_1170\_3.s\_g\_ULS] kN/m2

Ground snow load sg.SLS= [CCalcul\_1170\_3.s\_g\_SLS] kN/m2

Roof exposure category [ExposureCategory]

Exposure factor Ce = [CCalcul\_1170\_3.C\_e]

Factor μ1 = [CCalcul\_1170\_3.Nu1\_Alpha1]

Factor μ2 = [CCalcul\_1170\_3.Nu2\_Alpha1]

Roof snow load sULS= [CCalcul\_1170\_3.s\_ULS] kN/m2

Roof snow load sSLS= [CCalcul\_1170\_3.s\_SLS] kN/m2

## Wind Load

[WindLoad]

Annual probability of exceedance ULS: [AnnualProbabilityULS\_Wind]

Return period RULS.W = [R\_ULS\_Wind] years

Wind region [EWindRegion]

Terrain category [TerrainCategory]

Reference height z = [CCalcul\_1170\_2.z] m

Average structure height h = [CCalcul\_1170\_2.h] m

Regional 3s gust wind speed VR.ULS = [CCalcul\_1170\_2.V\_R\_ULS] m/s

Regional 3s gust wind speed VR.SLS = [CCalcul\_1170\_2.V\_R\_SLS] m/s

Terrain/height multiplier Mz.cat= [CCalcul\_1170\_2.M\_z\_cat]

Shielding multiplier Ms = [CCalcul\_1170\_2.M\_s]

Topographic multiplier Mt = [CCalcul\_1170\_2.M\_t]

Wind direction multiplier Md = [CCalcul\_1170\_2.fM\_D\_array\_values\_9[0]]

Site wind speed Vsit,β.ULS= [CCalcul\_1170\_2.V\_sit\_ULS\_Theta\_9[0]] m/s

Site wind speed Vsit,β.SLS= [CCalcul\_1170\_2.V\_sit\_SLS\_Theta\_9[0]] m/s

Design wind speed Vdes,θ.ULS=[CCalcul\_1170\_2.V\_des\_ULS\_Theta\_4[0]] m/s

Design wind speed Vdes,θ.SLS= [CCalcul\_1170\_2.V\_des\_SLS\_Theta\_4[0]] m/s

Density of air ρair = [CCalcul\_1170\_2.Rho\_air] kg/m3

Dynamic response factor Cdyn = [CCalcul\_1170\_2.C\_dyn]

Basic wind pressure pb.ULS = [CCalcul\_1170\_2.p\_basic\_ULS\_Theta\_4[0]] kN/m2

Basic wind pressure pb.SLS = [CCalcul\_1170\_2.p\_basic\_SLS\_Theta\_4[0]] kN/m2

## Seismic Load

Equivalent static method parameters

[SeismicLoad]

Annual probability of exceedance ULS: [AnnualProbabilityULS\_EQ]

Return period RULS.EQ = [R\_ULS\_EQ]

Site subsoil class [ESiteSubSoilClass]

Fault distance Dmin = [FaultDistanceDmin] km

Fault distance Dmax = [FaultDistanceDmax] km

Zone factor Z = [ZoneFactorZ]

Contributing weight Gtot.x= [CCalcul\_1170\_5.G\_tot\_x] kN

Contributing weight Gtot.y= [CCalcul\_1170\_5.G\_tot\_y] kN

Natural period along X-direction Tx = [CCalcul\_1170\_5.PeriodAlongYDirectionTx] s

Natural period along Y-direction Ty = [CCalcul\_1170\_5.PeriodAlongYDirectionTy] s

Spectral shape factor Ch(Tx) = [CCalcul\_1170\_5.SpectralShapeFactorChTx]

Spectral shape factor Ch(Ty) = [CCalcul\_1170\_5.SpectralShapeFactorChTy]

**ULS**

Structural ductility factor μ = [CCalcul\_1170\_5.Nu\_ULS]

Structural performance factor Sp = [CCalcul\_1170\_5.S\_p\_ULS\_strength]

Near-fault factor N(Tx,D) =[CCalcul\_1170\_5.N\_TxD\_ULS]

Elastic site hazard spectrum C(Tx) = [CCalcul\_1170\_5.C\_Tx\_ULS]

Factor kμ(Tx) = [CCalcul\_1170\_5.k\_Nu\_Tx\_ULS]

Horizontal design action coefficient Cd (Tx) = [CCalcul\_1170\_5.C\_d\_T1x\_ULS\_strength]

Horizontal static force Vx = [CCalcul\_1170\_5.V\_x\_ULS\_strength] kN

Near-fault factor N(Ty,D) =[CCalcul\_1170\_5.N\_TyD\_ULS]

Elastic site hazard spectrum C(Ty) = [CCalcul\_1170\_5.C\_Ty\_ULS]

Factor kμ(Ty) = [CCalcul\_1170\_5.k\_Nu\_Ty\_ULS]

Horizontal design action coefficient Cd (Ty) = [CCalcul\_1170\_5.C\_d\_T1y\_ULS\_strength]

Horizontal static force Vy = [CCalcul\_1170\_5.V\_y\_ULS\_strength] kN

**SLS**

Structural ductility factor μ = [CCalcul\_1170\_5.Nu\_SLS]

Structural performance factor Sp = [CCalcul\_1170\_5.S\_p\_SLS]

Near-fault factor N(Tx,D) =[CCalcul\_1170\_5.N\_TxD\_SLS]

Elastic site hazard spectrum C(Tx) = [CCalcul\_1170\_5.C\_Tx\_SLS]

Factor kμ(Tx) = [CCalcul\_1170\_5.k\_Nu\_Tx\_SLS]

Horizontal design action coefficient Cd (Tx) = [CCalcul\_1170\_5.C\_d\_T1x\_SLS]

Horizontal static force Vx = [CCalcul\_1170\_5.V\_x\_SLS] kN

Near-fault factor N(Ty,D) =[CCalcul\_1170\_5.N\_TyD\_SLS]

Elastic site hazard spectrum C(Ty) = [CCalcul\_1170\_5.C\_Ty\_SLS]

Factor kμ(Ty) = [CCalcul\_1170\_5.k\_Nu\_Ty\_SLS]

Horizontal design action coefficient Cd (Ty) = [CCalcul\_1170\_5.C\_d\_T1y\_SLS]

Horizontal static force Vy = [CCalcul\_1170\_5.V\_y\_SLS] kN

# Load Cases

[LoadCases]

# Load Combinations

[LoadCombinationsULS]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Limit State** | **Load Cases** | **Combination Key** | **Formula** |

[LoadCombinationsSLS]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Limit State** | **Load Cases** | **Combination Key** | **Formula** |

# Member design

[MemberDesign]

# Joint Design

[JointDesign]

## Member type: Main Column

Zobrazit pre kazdytypcombponenty so zaskrtnutym Design detailyposudkuspojov z UC\_JointDesign

TODO - Potrebovali by smetuvlozitobrazokspojanazaciatku a nakoncipruta v 3D alebo 2D.

Pre 2D by smemohlipouzit to canvas zo System Component Viewer



# Footing Design

TODO (oddelitvysledky od joint design)